<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="80.01" width="0" layer="20"/>
<wire x1="0" y1="80.01" x2="160.02" y2="80.01" width="0" layer="20"/>
<wire x1="160.02" y1="80.01" x2="160.02" y2="0" width="0" layer="20"/>
<wire x1="160.02" y1="0" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="76.2" drill="3.2"/>
<hole x="3.81" y="3.81" drill="3.2"/>
<hole x="156.21" y="3.81" drill="3.2"/>
<hole x="156.21" y="76.2" drill="3.2"/>
<text>PCB 11 * Ver. 1 * 12 / 2012</text>
<text>Egon Wanke &amp; Richo Andersen</text>
<text>Blitzortung.org</text>
</plain>
<libraries>
<library name="mc34063">
<description>&lt;b&gt;MC34063: 1.5 A, Step-Up/Down/Inverting Switching Regulator&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="0207/2V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 2.5 mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C050-030X075">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5 mm, outline 3 x 7.5 mm</description>
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="TJ3-U1">
<description>&lt;b&gt;Inductor&lt;/b&gt;&lt;p&gt;
Source: TJ-Serie Vishay.pdf</description>
</package>
<package name="0207/12">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 12 mm</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt; 0.3 inch</description>
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="556591-1">
<description>&lt;b&gt;Modular Jack&lt;/b&gt;&lt;p&gt;PC Board Ground</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<description>&lt;table width="100%" cellpadding="5" cellspacing="0"  bgcolor="#E0E0E0"&gt;
&lt;tr&gt;&lt;td&gt;
&lt;b&gt;Diodes&lt;/b&gt;&lt;br&gt;
Standard, Schottky, capacitance diodes, zener diodes, arrays, rectifiers, ... (&lt;b&gt;no&lt;/b&gt; optoelectronics)&lt;br&gt;
&lt;author&gt;&lt;b&gt;Update:&lt;/b&gt; 2009-06-19 Andreas Weidner&lt;/author&gt;
&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
&lt;br&gt;

&lt;b&gt;Device prefixes&lt;/b&gt;&lt;br&gt;
All devices have a dedicated prefix, sometimes followed by a 2-digit number, which signify
the component type and its grid spacing. The following components are available (excerpt):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;D[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DC[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Capacitance diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Diode rectifier&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DS[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Schottky diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DSB[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Bidirectional suppressor diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DSC[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Bidirectional crowbar suppressor diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DSU[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Unidirectional suppressor diode [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DZ[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Zener diode [length in 01"]&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Device suffixes&lt;/b&gt;&lt;br&gt;
Most devices offer different suffixes to directly specify either the solder pad or package type. The following suffixes are available (excerpt):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;(none)&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default package (often with normal pads, if available)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Device examples&lt;/b&gt;&lt;br&gt;
The following examples show devices that can be inserted into EAGLE schematics using
the &lt;b&gt;add&lt;/b&gt; command:&lt;p&gt; 
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;D&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default diode (currently 0.4" with normal pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DZ03R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Zener diode 0.3" with reduced pads&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;HSMS-2810&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Special Agilent diode with this name&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Board layers&lt;/b&gt;&lt;br&gt;
The board packages make special use of the following layers:&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tPlace,&lt;br&gt;&amp;nbsp;tNames,&lt;br&gt;&amp;nbsp;tValues&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Placeplan including device names and values for printed documentation. Should
    &lt;b&gt;not&lt;/b&gt; be used for the board imprint due to complexity. Names and values occupy
    the &lt;b&gt;same&lt;/b&gt; board space, so two separate printouts are advisable&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tDocu&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Less sophisticated, but concise placeplan with device names for the board imprint&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="D03N">
<description>&lt;b&gt;Diode&lt;/b&gt; 0.3"</description>
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="con-lumberg">
<description>&lt;b&gt;Lumberg Connectors&lt;/b&gt;&lt;p&gt;
include con-mfs.lbr - 2001.03.22&lt;br&gt;
Jack connectors - 2005.11.23&lt;p&gt;
http://www.lumberg.de&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1503_07">
<description>&lt;b&gt;Jack connectors according to JISC 6560, 3.5 mm&lt;/b&gt;&lt;p&gt;
Klinkensteckverbinder nach JISC 6560, 3,5 mm&lt;br&gt;
Source: http://www.lumberg.com/Produkte/PDFs/1503_07.pdf</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="32005-601">
<description>&lt;b&gt;MINI USB-B R/A DIP&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-601.pdf</description>
</package>
</packages>
</library>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSTBV2">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RN-5">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
<package name="RN-6">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="mc34063" package="DIL08" value="MC34063AP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="mc34063" package="DIL08" value="MC34063AP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="0207/10" value="0.47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="0207/10" value="180">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="0207/10" value="91k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="0207/10" value="13k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4-A" library="rcl" package="C025-025X050" value="270pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5-A" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1-A" library="diode" package="DO41-7.6" value="1N5819"/>
<element name="L2-A" library="rcl" package="TJ3-U1" value="100uH"/>
<element name="C7-A" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3-A" library="rcl" package="0207/2V" value="220uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6-A" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="0207/10" value="0.47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2-B" library="rcl" package="TJ3-U1" value="100uH"/>
<element name="D1-B" library="diode" package="DO41-7.6" value="1N5819"/>
<element name="C4-B" library="rcl" package="C025-025X050" value="270pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5-B" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3-B" library="rcl" package="0207/2V" value="220uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6-B" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7-B" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="0207/10" value="13k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="0207/10" value="91k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="0207/2V" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ATMEGA8" library="atmel" package="DIL28-3" value="MEGA8-P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CTRL" library="con-amp" package="556591-1" value="Controller">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="linear" package="DIL08" value="TL072">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC9" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC12" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22-A" library="rcl" package="0207/2V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24-A" library="rcl" package="0207/10" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23-A" library="rcl" package="0207/10" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8-A" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20-A" library="rcl" package="0207/10" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7-A" library="diode" package="DO41-7.6" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6-A" library="diode" package="DO41-7.6" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25-A" library="rcl" package="0207/2V" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10-A" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11-A" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31-A" library="rcl" package="0207/10" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30-A" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12-A" library="rcl" package="C050-030X075" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13-A" library="rcl" package="C050-030X075" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36-A" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37-A" library="rcl" package="0207/10" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21-A" library="rcl" package="0207/2V" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38-A" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39-A" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14-A" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15-A" library="rcl" package="C050-030X075" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16-A" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4-A" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5-A" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17-A" library="rcl" package="C025-025X050" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40-A" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10-A" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11-A" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41-A" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8-A" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9-A" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18-A" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44-A" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43-A" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42-A" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45-A" library="rcl" package="0207/10" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19-A" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="linear" package="DIL08" value="LM6172">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC11" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22-B" library="rcl" package="0207/2V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24-B" library="rcl" package="0207/10" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23-B" library="rcl" package="0207/10" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8-B" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20-B" library="rcl" package="0207/10" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7-B" library="diode" package="DO41-7.6" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6-B" library="diode" package="DO41-7.6" value="1N5819">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25-B" library="rcl" package="0207/2V" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10-B" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11-B" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31-B" library="rcl" package="0207/10" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="A30-B" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12-B" library="rcl" package="C050-030X075" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13-B" library="rcl" package="C050-030X075" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36-B" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37-B" library="rcl" package="0207/10" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21-B" library="rcl" package="0207/2V" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38-B" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39-B" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14-B" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15-B" library="rcl" package="C050-030X075" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16-B" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4-B" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5-B" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17-B" library="rcl" package="C025-025X050" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40-B" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10-B" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11-B" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41-B" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8-B" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9-B" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18-B" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44-B" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43-B" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42-B" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45-B" library="rcl" package="0207/10" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19-B" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="linear" package="DIL08" value="LM833N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="0207/2V" value="220"/>
<element name="R12" library="rcl" package="0207/10" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10-C" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11-C" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31-C" library="rcl" package="0207/10" value="3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30-C" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12-C" library="rcl" package="C050-030X075" value="470nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13-C" library="rcl" package="C050-030X075" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36-C" library="rcl" package="0207/10" value="3.6k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37-C" library="rcl" package="0207/10" value="390">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38-C" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39-C" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14-C" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15-C" library="rcl" package="C050-030X075" value="15nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16-C" library="rcl" package="C025-025X050" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4-C" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L5-C" library="rcl" package="0207/12" value="1mH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17-C" library="rcl" package="C025-025X050" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40-C" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10-C" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D11-C" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41-C" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8-C" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9-C" library="diode" package="DO41-7.6" value="BAT43">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18-C" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44-C" library="rcl" package="0207/10" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43-C" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42-C" library="rcl" package="0207/10" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45-C" library="rcl" package="0207/10" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19-C" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="0207/2V" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="0207/2V" value="10K"/>
<element name="R17" library="rcl" package="0207/2V" value="1.6k"/>
<element name="R13" library="rcl" package="0207/2V" value="22M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="0207/2V" value="22M"/>
<element name="IC4" library="burr-brown" package="DIL08" value="INA128P">
<attribute name="OC_NEWARK" value="74C9783"/>
<attribute name="MPN" value="INA128P"/>
<attribute name="MF" value="TEXAS INSTRUMENTS"/>
<attribute name="OC_FARNELL" value="1212410"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C38" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl" package="E5-10,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="diodes" package="D03N" value="1N4148">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D5" library="diodes" package="D03N" value="1N4148">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D3" library="diodes" package="D03N" value="1N4148">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="D2" library="diodes" package="D03N" value="1N4148">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
</element>
<element name="RESET" library="switch-omron" package="B3F-10XX" value="Reset">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
</element>
<element name="LED3" library="led" package="LED3MM" value="G1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="LED3MM" value="G2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="led" package="LED3MM" value="G3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="led" package="LED3MM" value="B1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="con-cypressindustries" package="32005-601" value="+5V">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35-C" library="rcl" package="0207/2V" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34-C" library="rcl" package="0207/2V" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33-C" library="rcl" package="0207/2V" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33-B" library="rcl" package="0207/2V" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35-B" library="rcl" package="0207/2V" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LINE-OUT" library="pinhead-1" package="1X05" value="line-out"/>
<element name="M-IN-1" library="con-phoenix-508" package="MSTBV2" value="MSTBV2">
<attribute name="OC_NEWARK" value="69R9845"/>
<attribute name="MPN" value="MSTBV 2,5/2-GF-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792792"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M-IN-2" library="con-phoenix-508" package="MSTBV2" value="MSTBV2">
<attribute name="OC_NEWARK" value="69R9845"/>
<attribute name="MPN" value="MSTBV 2,5/2-GF-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792792"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="E-IN" library="con-phoenix-508" package="MSTBV2" value="MSTBV2">
<attribute name="OC_NEWARK" value="69R9845"/>
<attribute name="MPN" value="MSTBV 2,5/2-GF-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792792"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29-A" library="rcl" package="0207/2V" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32-A" library="rcl" package="0207/2V" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33-A" library="rcl" package="0207/2V" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34-A" library="rcl" package="0207/2V" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9-B" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32-C" library="rcl" package="0207/2V" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28-C" library="rcl" package="0207/2V" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29-C" library="rcl" package="0207/2V" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9-A" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28-B" library="rcl" package="0207/2V" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29-B" library="rcl" package="0207/2V" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34-B" library="rcl" package="0207/2V" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32-B" library="rcl" package="0207/2V" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9-C" library="rcl" package="C050-030X075" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28-A" library="rcl" package="0207/2V" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35-A" library="rcl" package="0207/2V" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MP" library="pinhead-1" package="1X05" value="MP"/>
<element name="T2" library="switch-omron" package="B3F-10XX" value="T1">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="switch-omron" package="B3F-10XX" value="T2">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="switch-omron" package="B3F-10XX" value="T3">
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="led" package="LED5MM" value="G1"/>
<element name="R1" library="rcl" package="0207/10" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HEADSET" library="con-lumberg" package="1503_07" value="Headset">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R26-B" library="rcl" package="0207/2V" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26-A" library="rcl" package="0207/2V" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="0207/2V" value="5.6k"/>
<element name="GAIN-M1" library="pinhead-1" package="2X03" value="Gain M1"/>
<element name="GAIN-M2" library="pinhead-1" package="2X03" value="Gain M2"/>
<element name="GAIN-E" library="pinhead-1" package="2X03" value="Gain E"/>
<element name="R27-A" library="rcl" package="0207/2V" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27-B" library="rcl" package="0207/2V" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="0207/2V" value="499"/>
<element name="RN2" library="resistor-net" package="RN-5" value="10k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="G1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN1" library="resistor-net" package="RN-6" value="1k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C1" library="rcl" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="0207/2V" value="100"/>
<element name="R2" library="rcl" package="0207/2V" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="1"/>
<contactref element="L2-A" pad="2"/>
<contactref element="D1-A" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="8"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="IC1" pad="7"/>
<contactref element="R4" pad="2"/>
<contactref element="L2-A" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="3"/>
<contactref element="C4-A" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R7" pad="2"/>
<contactref element="D1-A" pad="C"/>
<contactref element="C5-A" pad="+"/>
<contactref element="L3-A" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="GND">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="C4-A" pad="2"/>
<contactref element="C5-A" pad="-"/>
<contactref element="C6-A" pad="2"/>
<contactref element="C7-A" pad="-"/>
<contactref element="C3" pad="-"/>
<contactref element="L2-B" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="C7-B" pad="+"/>
<contactref element="C6-B" pad="1"/>
<contactref element="C5-B" pad="+"/>
<contactref element="C2" pad="2"/>
<contactref element="ATMEGA8" pad="22"/>
<contactref element="ATMEGA8" pad="8"/>
<contactref element="CTRL" pad="G2"/>
<contactref element="CTRL" pad="G1"/>
<contactref element="CTRL" pad="5"/>
<contactref element="R24-A" pad="1"/>
<contactref element="D7-A" pad="A"/>
<contactref element="R30-A" pad="2"/>
<contactref element="R36-A" pad="2"/>
<contactref element="R21-A" pad="2"/>
<contactref element="R20-A" pad="1"/>
<contactref element="D6-A" pad="C"/>
<contactref element="C14-A" pad="1"/>
<contactref element="C15-A" pad="1"/>
<contactref element="C16-A" pad="1"/>
<contactref element="R39-A" pad="2"/>
<contactref element="R40-A" pad="2"/>
<contactref element="R42-A" pad="2"/>
<contactref element="R43-A" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="R24-B" pad="1"/>
<contactref element="D7-B" pad="A"/>
<contactref element="A30-B" pad="2"/>
<contactref element="R36-B" pad="2"/>
<contactref element="R21-B" pad="1"/>
<contactref element="R20-B" pad="1"/>
<contactref element="D6-B" pad="C"/>
<contactref element="C14-B" pad="1"/>
<contactref element="C15-B" pad="1"/>
<contactref element="C16-B" pad="1"/>
<contactref element="R39-B" pad="2"/>
<contactref element="R40-B" pad="2"/>
<contactref element="R42-B" pad="2"/>
<contactref element="R43-B" pad="2"/>
<contactref element="R30-C" pad="2"/>
<contactref element="R36-C" pad="2"/>
<contactref element="C14-C" pad="1"/>
<contactref element="C15-C" pad="1"/>
<contactref element="C16-C" pad="1"/>
<contactref element="R39-C" pad="2"/>
<contactref element="R40-C" pad="2"/>
<contactref element="R42-C" pad="2"/>
<contactref element="R43-C" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C39" pad="-"/>
<contactref element="C38" pad="-"/>
<contactref element="R14" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="IC4" pad="5"/>
<contactref element="+5V" pad="5"/>
<contactref element="C35" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="M-IN-2" pad="2"/>
<contactref element="M-IN-1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="HEADSET" pad="1"/>
<contactref element="T2" pad="3"/>
<contactref element="T1" pad="3"/>
<contactref element="MP" pad="2"/>
<contactref element="MP" pad="4"/>
<contactref element="T3" pad="3"/>
<contactref element="RESET" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="2"/>
<contactref element="L2-B" pad="1"/>
<contactref element="D1-B" pad="C"/>
</signal>
<signal name="N$12">
<contactref element="IC2" pad="3"/>
<contactref element="C4-B" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="4"/>
<contactref element="C4-B" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="L3-B" pad="1"/>
<contactref element="D1-B" pad="A"/>
<contactref element="C5-B" pad="-"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$16">
<contactref element="ATMEGA8" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="CTRL" pad="3"/>
<contactref element="CTRL" pad="6"/>
<contactref element="L1" pad="2"/>
<contactref element="+5V" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="CTRL" pad="4"/>
<contactref element="C19-B" pad="2"/>
<contactref element="LINE-OUT" pad="5"/>
<contactref element="MP" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="IC6" pad="2"/>
<contactref element="R23-A" pad="2"/>
<contactref element="C8-A" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="IC6" pad="3"/>
<contactref element="R24-A" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="IC6" pad="1"/>
<contactref element="R22-A" pad="2"/>
<contactref element="C8-A" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R22-A" pad="1"/>
<contactref element="R21-A" pad="1"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="D7-A" pad="C"/>
<contactref element="D6-A" pad="A"/>
<contactref element="R20-A" pad="2"/>
<contactref element="IC5" pad="2"/>
<contactref element="M-IN-1" pad="1"/>
<contactref element="R25-A" pad="1"/>
<contactref element="R26-A" pad="1"/>
<contactref element="R27-A" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="C10-A" pad="2"/>
<contactref element="C11-A" pad="1"/>
<contactref element="R31-A" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="C11-A" pad="2"/>
<contactref element="IC9" pad="3"/>
<contactref element="R30-A" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="IC9" pad="1"/>
<contactref element="R31-A" pad="1"/>
<contactref element="IC9" pad="2"/>
<contactref element="C12-A" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C12-A" pad="2"/>
<contactref element="C13-A" pad="1"/>
<contactref element="R37-A" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="C13-A" pad="2"/>
<contactref element="R36-A" pad="1"/>
<contactref element="IC9" pad="5"/>
</signal>
<signal name="N$32">
<contactref element="IC9" pad="6"/>
<contactref element="IC9" pad="7"/>
<contactref element="R37-A" pad="1"/>
<contactref element="R38-A" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="C17-A" pad="2"/>
<contactref element="R39-A" pad="1"/>
<contactref element="IC12" pad="3"/>
</signal>
<signal name="N$34">
<contactref element="L5-A" pad="2"/>
<contactref element="C17-A" pad="1"/>
<contactref element="C16-A" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="L4-A" pad="2"/>
<contactref element="L5-A" pad="1"/>
<contactref element="C15-A" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="R38-A" pad="1"/>
<contactref element="L4-A" pad="1"/>
<contactref element="C14-A" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="R40-A" pad="1"/>
<contactref element="IC12" pad="2"/>
<contactref element="R41-A" pad="2"/>
<contactref element="D8-A" pad="A"/>
<contactref element="D9-A" pad="C"/>
</signal>
<signal name="N$38">
<contactref element="IC12" pad="1"/>
<contactref element="R41-A" pad="1"/>
<contactref element="D8-A" pad="C"/>
<contactref element="C18-A" pad="1"/>
<contactref element="D9-A" pad="A"/>
</signal>
<signal name="N$39">
<contactref element="C18-A" pad="2"/>
<contactref element="R42-A" pad="1"/>
<contactref element="IC12" pad="5"/>
</signal>
<signal name="N$40">
<contactref element="R43-A" pad="1"/>
<contactref element="IC12" pad="6"/>
<contactref element="R44-A" pad="2"/>
<contactref element="D10-A" pad="A"/>
<contactref element="D11-A" pad="C"/>
</signal>
<signal name="D10-A">
<contactref element="IC12" pad="7"/>
<contactref element="R44-A" pad="1"/>
<contactref element="D10-A" pad="C"/>
<contactref element="D11-A" pad="A"/>
<contactref element="R45-A" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="R45-A" pad="2"/>
<contactref element="C19-A" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="C19-A" pad="2"/>
<contactref element="CTRL" pad="7"/>
<contactref element="LINE-OUT" pad="1"/>
<contactref element="MP" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="R23-B" pad="2"/>
<contactref element="C8-B" pad="2"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$46">
<contactref element="R22-B" pad="1"/>
<contactref element="C8-B" pad="1"/>
<contactref element="IC6" pad="7"/>
</signal>
<signal name="N$47">
<contactref element="R22-B" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="R21-B" pad="2"/>
</signal>
<signal name="N$50">
<contactref element="C10-B" pad="2"/>
<contactref element="C11-B" pad="1"/>
<contactref element="R31-B" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="C11-B" pad="2"/>
<contactref element="IC8" pad="3"/>
<contactref element="A30-B" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="IC8" pad="1"/>
<contactref element="R31-B" pad="1"/>
<contactref element="IC8" pad="2"/>
<contactref element="C12-B" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="C12-B" pad="2"/>
<contactref element="C13-B" pad="1"/>
<contactref element="R37-B" pad="2"/>
</signal>
<signal name="C13-B">
<contactref element="C13-B" pad="2"/>
<contactref element="R36-B" pad="1"/>
<contactref element="IC8" pad="5"/>
</signal>
<signal name="N$55">
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="7"/>
<contactref element="R37-B" pad="1"/>
<contactref element="R38-B" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="C17-B" pad="2"/>
<contactref element="R39-B" pad="1"/>
<contactref element="IC11" pad="3"/>
</signal>
<signal name="N$57">
<contactref element="L5-B" pad="2"/>
<contactref element="C17-B" pad="1"/>
<contactref element="C16-B" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="L4-B" pad="2"/>
<contactref element="L5-B" pad="1"/>
<contactref element="C15-B" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="R38-B" pad="1"/>
<contactref element="L4-B" pad="1"/>
<contactref element="C14-B" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="R40-B" pad="1"/>
<contactref element="IC11" pad="2"/>
<contactref element="R41-B" pad="2"/>
<contactref element="D8-B" pad="A"/>
<contactref element="D9-B" pad="C"/>
</signal>
<signal name="N$61">
<contactref element="IC11" pad="1"/>
<contactref element="R41-B" pad="1"/>
<contactref element="D8-B" pad="C"/>
<contactref element="C18-B" pad="1"/>
<contactref element="D9-B" pad="A"/>
</signal>
<signal name="N$62">
<contactref element="C18-B" pad="2"/>
<contactref element="R42-B" pad="1"/>
<contactref element="IC11" pad="5"/>
</signal>
<signal name="N$63">
<contactref element="R43-B" pad="1"/>
<contactref element="IC11" pad="6"/>
<contactref element="R44-B" pad="2"/>
<contactref element="D10-B" pad="A"/>
<contactref element="D11-B" pad="C"/>
</signal>
<signal name="N$64">
<contactref element="IC11" pad="7"/>
<contactref element="R44-B" pad="1"/>
<contactref element="D10-B" pad="C"/>
<contactref element="D11-B" pad="A"/>
<contactref element="R45-B" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R45-B" pad="2"/>
<contactref element="C19-B" pad="1"/>
</signal>
<signal name="N$73">
<contactref element="C10-C" pad="2"/>
<contactref element="C11-C" pad="1"/>
<contactref element="R31-C" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="C11-C" pad="2"/>
<contactref element="IC7" pad="3"/>
<contactref element="R30-C" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="C12-C" pad="2"/>
<contactref element="C13-C" pad="1"/>
<contactref element="R37-C" pad="2"/>
</signal>
<signal name="N$77">
<contactref element="C13-C" pad="2"/>
<contactref element="R36-C" pad="1"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$78">
<contactref element="IC7" pad="6"/>
<contactref element="IC7" pad="7"/>
<contactref element="R37-C" pad="1"/>
<contactref element="R38-C" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="C17-C" pad="2"/>
<contactref element="R39-C" pad="1"/>
<contactref element="IC10" pad="3"/>
</signal>
<signal name="N$80">
<contactref element="L5-C" pad="2"/>
<contactref element="C17-C" pad="1"/>
<contactref element="C16-C" pad="2"/>
</signal>
<signal name="N$81">
<contactref element="L4-C" pad="2"/>
<contactref element="L5-C" pad="1"/>
<contactref element="C15-C" pad="2"/>
</signal>
<signal name="N$82">
<contactref element="R38-C" pad="1"/>
<contactref element="L4-C" pad="1"/>
<contactref element="C14-C" pad="2"/>
</signal>
<signal name="N$83">
<contactref element="R40-C" pad="1"/>
<contactref element="IC10" pad="2"/>
<contactref element="R41-C" pad="2"/>
<contactref element="D8-C" pad="A"/>
<contactref element="D9-C" pad="C"/>
</signal>
<signal name="N$84">
<contactref element="IC10" pad="1"/>
<contactref element="R41-C" pad="1"/>
<contactref element="D8-C" pad="C"/>
<contactref element="C18-C" pad="1"/>
<contactref element="D9-C" pad="A"/>
</signal>
<signal name="N$85">
<contactref element="C18-C" pad="2"/>
<contactref element="R42-C" pad="1"/>
<contactref element="IC10" pad="5"/>
</signal>
<signal name="N$86">
<contactref element="R43-C" pad="1"/>
<contactref element="IC10" pad="6"/>
<contactref element="R44-C" pad="2"/>
<contactref element="D10-C" pad="A"/>
<contactref element="D11-C" pad="C"/>
</signal>
<signal name="N$87">
<contactref element="IC10" pad="7"/>
<contactref element="R44-C" pad="1"/>
<contactref element="D10-C" pad="C"/>
<contactref element="D11-C" pad="A"/>
<contactref element="R45-C" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="R45-C" pad="2"/>
<contactref element="C19-C" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="C19-C" pad="2"/>
<contactref element="CTRL" pad="1"/>
<contactref element="LINE-OUT" pad="3"/>
<contactref element="MP" pad="3"/>
</signal>
<signal name="N$105">
<contactref element="R17" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="R19" pad="1"/>
<contactref element="IC4" pad="3"/>
<contactref element="D5" pad="A"/>
<contactref element="D3" pad="C"/>
</signal>
<signal name="N$109">
<contactref element="R14" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="E-IN" pad="2"/>
</signal>
<signal name="N$111">
<contactref element="R13" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="E-IN" pad="1"/>
</signal>
<signal name="V--">
<contactref element="IC4" pad="4"/>
<contactref element="R11" pad="1"/>
<contactref element="D3" pad="A"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$107">
<contactref element="IC4" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="V-">
<contactref element="R11" pad="2"/>
<contactref element="L3-B" pad="2"/>
<contactref element="C6-B" pad="2"/>
<contactref element="C7-B" pad="-"/>
<contactref element="IC6" pad="4"/>
<contactref element="C21" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="C29" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="IC9" pad="4"/>
<contactref element="IC12" pad="4"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC11" pad="4"/>
<contactref element="IC7" pad="4"/>
<contactref element="IC10" pad="4"/>
<contactref element="C37" pad="1"/>
<contactref element="C39" pad="+"/>
<contactref element="C35" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="6"/>
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="C3" pad="+"/>
<contactref element="L1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="ATMEGA8" pad="7"/>
<contactref element="ATMEGA8" pad="21"/>
<contactref element="ATMEGA8" pad="20"/>
<contactref element="RN2" pad="1"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="V+">
<contactref element="R28-B" pad="1"/>
<contactref element="R28-A" pad="1"/>
<contactref element="R28-C" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="C38" pad="+"/>
<contactref element="L3-A" pad="1"/>
<contactref element="C6-A" pad="1"/>
<contactref element="C7-A" pad="+"/>
<contactref element="IC6" pad="8"/>
<contactref element="C20" pad="1"/>
<contactref element="IC9" pad="8"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC11" pad="8"/>
<contactref element="IC7" pad="8"/>
<contactref element="IC10" pad="8"/>
<contactref element="C32" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C28" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C36" pad="1"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="N$124">
<contactref element="LINE-OUT" pad="4"/>
<contactref element="HEADSET" pad="2@1"/>
</signal>
<signal name="N$125">
<contactref element="LINE-OUT" pad="2"/>
<contactref element="HEADSET" pad="3"/>
</signal>
<signal name="N$45">
<contactref element="R24-B" pad="2"/>
<contactref element="IC6" pad="5"/>
</signal>
<signal name="N$66">
<contactref element="C12-C" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="R31-C" pad="1"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$91">
<contactref element="CTRL" pad="8"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="V++">
<contactref element="IC4" pad="7"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$113">
<contactref element="ATMEGA8" pad="17"/>
<contactref element="R33-C" pad="1"/>
</signal>
<signal name="N$114">
<contactref element="R34-C" pad="1"/>
<contactref element="ATMEGA8" pad="16"/>
</signal>
<signal name="N$49">
<contactref element="R32-C" pad="1"/>
<contactref element="ATMEGA8" pad="18"/>
</signal>
<signal name="N$117">
<contactref element="R35-C" pad="1"/>
<contactref element="ATMEGA8" pad="15"/>
</signal>
<signal name="N$93">
<contactref element="R35-A" pad="1"/>
<contactref element="ATMEGA8" pad="14"/>
</signal>
<signal name="N$94">
<contactref element="R34-A" pad="1"/>
<contactref element="ATMEGA8" pad="13"/>
</signal>
<signal name="N$99">
<contactref element="LED5" pad="K"/>
<contactref element="ATMEGA8" pad="5"/>
</signal>
<signal name="N$100">
<contactref element="LED6" pad="K"/>
<contactref element="ATMEGA8" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="R29-B" pad="1"/>
<contactref element="R33-B" pad="2"/>
<contactref element="R35-B" pad="2"/>
<contactref element="R34-B" pad="2"/>
<contactref element="R32-B" pad="2"/>
<contactref element="C10-B" pad="1"/>
</signal>
<signal name="N$102">
<contactref element="R23-B" pad="1"/>
<contactref element="IC5" pad="7"/>
<contactref element="C9-B" pad="2"/>
<contactref element="GAIN-M2" pad="2"/>
<contactref element="GAIN-M2" pad="4"/>
<contactref element="GAIN-M2" pad="6"/>
</signal>
<signal name="N$120">
<contactref element="R23-A" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="C9-A" pad="2"/>
<contactref element="GAIN-M1" pad="2"/>
<contactref element="GAIN-M1" pad="4"/>
<contactref element="GAIN-M1" pad="6"/>
</signal>
<signal name="N$101">
<contactref element="R29-A" pad="1"/>
<contactref element="R32-A" pad="2"/>
<contactref element="R33-A" pad="2"/>
<contactref element="R34-A" pad="2"/>
<contactref element="R35-A" pad="2"/>
<contactref element="C10-A" pad="1"/>
</signal>
<signal name="N$106">
<contactref element="IC5" pad="6"/>
<contactref element="D7-B" pad="C"/>
<contactref element="D6-B" pad="A"/>
<contactref element="R20-B" pad="2"/>
<contactref element="M-IN-2" pad="1"/>
<contactref element="R25-B" pad="1"/>
<contactref element="R26-B" pad="1"/>
<contactref element="R27-B" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C9-B" pad="1"/>
<contactref element="R29-B" pad="2"/>
<contactref element="R28-B" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="R32-B" pad="1"/>
<contactref element="ATMEGA8" pad="25"/>
</signal>
<signal name="N$27">
<contactref element="R34-B" pad="1"/>
<contactref element="ATMEGA8" pad="23"/>
</signal>
<signal name="N$48">
<contactref element="R35-B" pad="1"/>
<contactref element="ATMEGA8" pad="19"/>
</signal>
<signal name="N$71">
<contactref element="R33-B" pad="1"/>
<contactref element="ATMEGA8" pad="24"/>
</signal>
<signal name="N$68">
<contactref element="IC4" pad="6"/>
<contactref element="C9-C" pad="2"/>
</signal>
<signal name="N$69">
<contactref element="LED3" pad="K"/>
<contactref element="ATMEGA8" pad="27"/>
</signal>
<signal name="N$72">
<contactref element="LED4" pad="K"/>
<contactref element="ATMEGA8" pad="4"/>
</signal>
<signal name="N$98">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$119">
<contactref element="R32-A" pad="1"/>
<contactref element="ATMEGA8" pad="11"/>
</signal>
<signal name="N$95">
<contactref element="ATMEGA8" pad="12"/>
<contactref element="R33-A" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="R25-B" pad="2"/>
<contactref element="GAIN-M2" pad="1"/>
</signal>
<signal name="N$97">
<contactref element="R26-B" pad="2"/>
<contactref element="GAIN-M2" pad="3"/>
</signal>
<signal name="N$110">
<contactref element="R26-A" pad="2"/>
<contactref element="GAIN-M1" pad="3"/>
</signal>
<signal name="N$103">
<contactref element="R25-A" pad="2"/>
<contactref element="GAIN-M1" pad="1"/>
</signal>
<signal name="N$112">
<contactref element="R17" pad="2"/>
<contactref element="GAIN-E" pad="3"/>
</signal>
<signal name="N$75">
<contactref element="R18" pad="2"/>
<contactref element="GAIN-E" pad="1"/>
</signal>
<signal name="N$115">
<contactref element="IC4" pad="8"/>
<contactref element="GAIN-E" pad="2"/>
<contactref element="GAIN-E" pad="4"/>
<contactref element="GAIN-E" pad="6"/>
</signal>
<signal name="N$116">
<contactref element="R27-A" pad="2"/>
<contactref element="GAIN-M1" pad="5"/>
</signal>
<signal name="N$123">
<contactref element="R27-B" pad="2"/>
<contactref element="GAIN-M2" pad="5"/>
</signal>
<signal name="N$127">
<contactref element="R16" pad="2"/>
<contactref element="GAIN-E" pad="5"/>
</signal>
<signal name="N$121">
<contactref element="R29-C" pad="1"/>
<contactref element="R32-C" pad="2"/>
<contactref element="R35-C" pad="2"/>
<contactref element="R34-C" pad="2"/>
<contactref element="R33-C" pad="2"/>
<contactref element="C10-C" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R29-C" pad="2"/>
<contactref element="C9-C" pad="1"/>
<contactref element="R28-C" pad="2"/>
</signal>
<signal name="N$67">
<contactref element="T1" pad="1"/>
<contactref element="ATMEGA8" pad="9"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="N$118">
<contactref element="T2" pad="1"/>
<contactref element="ATMEGA8" pad="10"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="RESET" pad="1"/>
<contactref element="ATMEGA8" pad="1"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="N$130">
<contactref element="T3" pad="1"/>
<contactref element="ATMEGA8" pad="26"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="N$128">
<contactref element="R28-A" pad="2"/>
<contactref element="R29-A" pad="2"/>
<contactref element="C9-A" pad="1"/>
</signal>
<signal name="N$126">
<contactref element="LED2" pad="K"/>
<contactref element="ATMEGA8" pad="28"/>
</signal>
<signal name="N$90">
<contactref element="LED2" pad="A"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$92">
<contactref element="LED3" pad="A"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$104">
<contactref element="LED4" pad="A"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$122">
<contactref element="LED5" pad="A"/>
<contactref element="RN1" pad="6"/>
</signal>
<signal name="N$129">
<contactref element="LED6" pad="A"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$131">
<contactref element="ATMEGA8" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$132">
<contactref element="CTRL" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
