<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="120.015" y2="0" width="0" layer="20"/>
<wire x1="120.015" y1="0" x2="120.015" y2="96.52" width="0" layer="20"/>
<wire x1="120.015" y1="96.52" x2="0" y2="96.52" width="0" layer="20"/>
<wire x1="0" y1="96.52" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="92.71" drill="3.2"/>
<hole x="3.81" y="3.81" drill="3.2"/>
<hole x="116.205" y="8.89" drill="3.2"/>
<hole x="116.205" y="92.71" drill="3.2"/>
<text>PCB 10 * Ver. 5 * 4/2014</text>
<text>www.Blitzortung.org</text>
<text>Egon Wanke &amp;</text>
<text>Tobias Volgnandt</text>
<text>GND</text>
<text>S RX</text>
<text>S TX</text>
<text>+3V3</text>
<text>+5V</text>
<text>FGPMMOPA6H</text>
<text>green</text>
<text>MP</text>
</plain>
<libraries>
<library name="pinhead-1">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X25">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
<package name="1X05/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="1X02/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54 90°</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="microchip-enc28j60">
<description>Microchip ENC28J60 Ethernet contoller with SPI interface.</description>
<packages>
<package name="DIL28-3">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;&lt;p&gt;
package type P</description>
</package>
</packages>
</library>
<library name="con-amp">
<description>&lt;b&gt;AMP Connectors&lt;/b&gt;&lt;p&gt;
RJ45 Jack connectors&lt;br&gt;
 Based on the previous libraris:
 &lt;ul&gt;
 &lt;li&gt;amp.lbr
 &lt;li&gt;amp-j.lbr
 &lt;li&gt;amp-mta.lbr
 &lt;li&gt;amp-nlok.lbr
 &lt;li&gt;amp-sim.lbr
 &lt;li&gt;amp-micro-match.lbr
 &lt;/ul&gt;
 Sources :
 &lt;ul&gt;
 &lt;li&gt;Catalog 82066 Revised 11-95 
 &lt;li&gt;Product Guide 296785 Rev. 8-99
 &lt;li&gt;Product Guide CD-ROM 1999
 &lt;li&gt;www.amp.com
 &lt;/ul&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="556591-1">
<description>&lt;b&gt;Modular Jack&lt;/b&gt;&lt;p&gt;PC Board Ground</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="32005-601">
<description>&lt;b&gt;MINI USB-B R/A DIP&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-601.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="0207/15">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 15mm</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="E5-8,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 8.5 mm</description>
</package>
<package name="E2,5-6">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 6 mm</description>
</package>
</packages>
</library>
<library name="ic">
<description>&lt;table width="100%" cellpadding="5" cellspacing="0"  bgcolor="#E0E0E0"&gt;
&lt;tr&gt;&lt;td&gt;
&lt;b&gt;Special Integrated Circuits&lt;/b&gt;&lt;br&gt;
Voltage regulators, analog switches, interface drivers, multiplexers, mixers, phase shifters, DC/DC converters, ...&lt;br&gt;
&lt;author&gt;&lt;b&gt;Update:&lt;/b&gt; 2009-07-27 Andreas Weidner&lt;/author&gt;
&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
&lt;br&gt;

&lt;b&gt;IC suffixes&lt;/b&gt;&lt;br&gt;
Most ICs offer different suffixes to directly specify the package type. In general, these are
&lt;b&gt;not&lt;/b&gt; the manufacturer's suffixes (they vary greatly), but one of the following (note that not all ICs offer all types of packages):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;(none)&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default IC package (currently DIP with long pads, if available)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIP package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;L&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIP package with long pads (easily solderable, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIP package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;S&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SMD package&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;IC examples&lt;/b&gt;&lt;br&gt;
The following examples show devices that can be inserted into EAGLE schematics using
the &lt;b&gt;add&lt;/b&gt; command:&lt;p&gt; 
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;AD587&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;10V voltage reference in default package (currently DIP-8 with long pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;NE555R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Timer in DIP-8 package with reduced pads&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;ADG451S&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Quad analog switch in SO-16 SMD package&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Board layers&lt;/b&gt;&lt;br&gt;
The board packages make special use of the following layers:&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tPlace,&lt;br&gt;&amp;nbsp;tNames,&lt;br&gt;&amp;nbsp;tValues&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Placeplan including device names and values for printed documentation. Should
    &lt;b&gt;not&lt;/b&gt; be used for the board imprint due to complexity. Names and values occupy
    the &lt;b&gt;same&lt;/b&gt; board space, so two separate printouts are advisable&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tDocu&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Less sophisticated, but concise placeplan with device names for the board imprint&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="TO220L">
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49U-V">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO92-EBC">
<description>&lt;b&gt;TO-92&lt;/b&gt;&lt;p&gt;
 grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="con-ml">
<description>&lt;b&gt;Harting  Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML6">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Simple Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X09M">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2MM"</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/CM12P">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="itead_BP_110825.lbr">
<packages>
<package name="HR911105A">
</package>
</packages>
</library>
<library name="resistor-net">
<description>&lt;b&gt;Generic Resistor Networks&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RN-9">
<description>&lt;b&gt;RESISTOR NETWORK&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor-sil">
<description>&lt;b&gt;Resistors in Single Inline Packages&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIL12">
<description>&lt;b&gt;Single In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="LIB-FGPMMOPA6H_PA6H">
<description>GlobalTop GPS Receiver PA6H</description>
<packages>
<package name="FGPMMOPA6H">
</package>
</packages>
</library>
<library name="connectors">
<description>&lt;table width="100%" cellpadding="5" cellspacing="0"  bgcolor="#E0E0E0"&gt;
&lt;tr&gt;&lt;td&gt;
&lt;b&gt;Connectors&lt;/b&gt;&lt;br&gt;
Connectors, screw + crimp terminals, jumpers, test points, pins, pads, ...&lt;br&gt;
&lt;author&gt;&lt;b&gt;Update:&lt;/b&gt; 2009-07-02 Andreas Weidner&lt;/author&gt;
&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
&lt;br&gt;

&lt;b&gt;Device prefixes&lt;/b&gt;&lt;br&gt;
All devices have a dedicated prefix, sometimes followed by a 2-digit number, which signify
the connector type and its pin number. The following device types are available (excerpt):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;J[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Jumper [length in 0.1"]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;JP[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Jumper pin block [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;X[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XA[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector with alternating pins [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XB[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Backplane connector [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XC&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Crimp terminal for shielded cables&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XD&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Digital ground test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XG&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Ground test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XP&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Input/output pin&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XS&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Shielded connector&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XT&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Test point&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XU[Nr]&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Connector with unconnected (separate) pins [pin number]&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Connector suffixes&lt;/b&gt;&lt;br&gt;
Most connectors offer different suffixes to directly specify the package type. The following list gives some
examples of available suffixes (note that not all connectors offer all types of packages):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;(none)&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default connector package (currently DIL with normal pads, if available)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;D&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIL package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;DR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;DIL package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;I&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;IDC package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;IR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;IDC package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;L&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with long pads (easily solderable, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with normal pads (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;SIL package with reduced pads (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Pin suffixes&lt;/b&gt;&lt;br&gt;
Most input/output pins offer different suffixes to directly specify the pad type. The following suffixes
are available (note that not all pins offer all types of pads):&lt;p&gt;
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;N &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Normal pad (easily solderable)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;L &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Long pad (easily solderable, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;R &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Reduced pad (small, through-pin-routing possible)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;B &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Big pad (0.1")&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;H &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Huge pad (0.15")&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;M &lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Maximised pad (0.2")&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Device examples&lt;/b&gt;&lt;br&gt;
The following examples show devices that can be inserted into EAGLE schematics using
the &lt;b&gt;add&lt;/b&gt; command:&lt;p&gt; 
&lt;table border="0" cellpadding="0" cellspacing="0"&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;J&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default jumper (currently 0.2" with normal pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;X06&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default 6-pin connector (currently DIL package with normal pads)&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XA16IR&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;16-pin connector with alternating pins in IDC package with reduced pads&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XC&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Default crimp terminal for shielded cables&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;XPL&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Input/output pin with long pads&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;hr&gt;

&lt;b&gt;Board layers&lt;/b&gt;&lt;br&gt;
The board packages make special use of the following layers:&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tPlace,&lt;br&gt;&amp;nbsp;tNames,&lt;br&gt;&amp;nbsp;tValues&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Placeplan including device names and values for printed documentation. Should
    &lt;b&gt;not&lt;/b&gt; be used for the board imprint due to complexity. Names and values occupy
    the &lt;b&gt;same&lt;/b&gt; board space, so two separate printouts are advisable&lt;/td&gt;
&lt;/tr&gt;
&lt;tr&gt;
  &lt;td&gt;&lt;tt&gt;tDocu&lt;/tt&gt;&lt;/td&gt;
  &lt;td&gt;Less sophisticated, but concise placeplan with device names for the board imprint&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="XS-SMA01">
<description>&lt;b&gt;SMA connector&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="con-phoenix-508">
<description>&lt;b&gt;Phoenix Connectors&lt;/b&gt;&lt;p&gt;
Grid 5.08 mm&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;pho508a.lbr
&lt;li&gt;pho508b.lbr
&lt;li&gt;pho508c.lbr
&lt;li&gt;pho508d.lbr
&lt;li&gt;pho508e.lbr
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MSTBV2">
<description>&lt;b&gt;PHOENIX&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P1" library="pinhead-1" package="2X25" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="pinhead-1" package="2X25" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ENC28J60" library="microchip-enc28j60" package="DIL28-3" value="ENC28J60">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN1" library="con-amp" package="556591-1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+5VDC," library="con-cypressindustries" package="32005-601" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="0207/10" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rcl" package="0207/10" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="0207/10" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rcl" package="0207/10" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rcl" package="0207/10" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="rcl" package="0207/10" value="49.9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl" package="C025-024X044" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="C025-024X044" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="0207/10" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LF33CV" library="ic" package="TO220L" value=""/>
<element name="C47" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="E2,5-6" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="E2,5-6" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L40" library="rcl" package="0207/15" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="25MHZ" library="crystal" package="HC49U-V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1666969"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IN2" library="con-amp" package="556591-1" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rcl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T40" library="transistor-npn" package="TO92-EBC" value="BC338">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="rcl" package="0207/10" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="rcl" package="E2,5-6" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="rcl" package="E2,5-6" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="EM-406A" library="con-ml" package="ML6" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="rcl" package="0207/10" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BUZZER" library="buzzer" package="F/CM12P" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T41" library="transistor-npn" package="TO92-EBC" value="BC338">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="rcl" package="0207/10" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HR911105A" library="itead_BP_110825.lbr" package="HR911105A" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D47" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D45" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D41" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D49" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D43" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D46" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D44" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D40" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D50" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D48" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D42" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D51" library="diode" package="DO35-7" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C61" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN42" library="resistor-net" package="RN-9" value="10K">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RN40" library="resistor-net" package="RN-9" value="100">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RN41" library="resistor-sil" package="SIL12" value="1k">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FGPMMOPA6H" library="LIB-FGPMMOPA6H_PA6H" package="FGPMMOPA6H" value=""/>
<element name="GPS-ANT" library="connectors" package="XS-SMA01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1-9" library="pinhead" package="1X09M" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="10-18" library="pinhead" package="1X09M" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="rcl" package="0207/10" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="rcl" package="0207/10" value="2.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C59" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C60" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D55" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D56" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D54" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D57" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPS-FIX" library="led" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="rcl" package="0207/10" value="680">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="E5-8,5" value="470uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="rcl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="rcl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="rcl" package="0207/10" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R59" library="rcl" package="0207/10" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="rcl" package="0207/10" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="rcl" package="0207/10" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L41" library="rcl" package="0207/15" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L42" library="rcl" package="0207/15" value="10uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead-1" package="1X02/90" value="">
<attribute name="VALUE"/>
</element>
<element name="R48" library="rcl" package="0207/10" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R49" library="rcl" package="0207/10" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D53" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SERIEL" library="pinhead-1" package="1X05/90" value=""/>
<element name="R62" library="rcl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R63" library="rcl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GROUND" library="con-phoenix-508" package="MSTBV2" value="">
<attribute name="OC_NEWARK" value="69R9845"/>
<attribute name="MPN" value="MSTBV 2,5/2-GF-5.08"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1792792"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="rcl" package="0207/10" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="rcl" package="0207/10" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D58" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D59" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C63" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="rcl" package="C025-024X044" value="220nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D52" library="diode" package="DO35-7" value="1N5818">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C64" library="rcl" package="C025-024X044" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOD1016" library="pinhead-1" package="1X07" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="C41" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C43" pad="1"/>
<contactref element="C40" pad="2"/>
<contactref element="ENC28J60" pad="11"/>
<contactref element="ENC28J60" pad="21"/>
<contactref element="ENC28J60" pad="18"/>
<contactref element="ENC28J60" pad="22"/>
<contactref element="ENC28J60" pad="2"/>
<contactref element="LF33CV" pad="2"/>
<contactref element="C44" pad="-"/>
<contactref element="R46" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="LF33CV" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C48" pad="-"/>
<contactref element="P1" pad="1"/>
<contactref element="P1" pad="49"/>
<contactref element="P1" pad="50"/>
<contactref element="P1" pad="2"/>
<contactref element="P1" pad="5"/>
<contactref element="P2" pad="49"/>
<contactref element="P2" pad="1"/>
<contactref element="P2" pad="2"/>
<contactref element="P2" pad="50"/>
<contactref element="P1" pad="23"/>
<contactref element="T40" pad="E"/>
<contactref element="C55" pad="-"/>
<contactref element="IN1" pad="5"/>
<contactref element="T41" pad="E"/>
<contactref element="IN2" pad="5"/>
<contactref element="EM-406A" pad="5"/>
<contactref element="HR911105A" pad="GND"/>
<contactref element="HR911105A" pad="SHIELD0"/>
<contactref element="HR911105A" pad="SHIELD1"/>
<contactref element="HR911105A" pad="Y-"/>
<contactref element="HR911105A" pad="G-"/>
<contactref element="D46" pad="A"/>
<contactref element="D44" pad="A"/>
<contactref element="D40" pad="A"/>
<contactref element="D50" pad="A"/>
<contactref element="D48" pad="A"/>
<contactref element="D42" pad="A"/>
<contactref element="IN2" pad="G2"/>
<contactref element="IN2" pad="G1"/>
<contactref element="IN1" pad="G2"/>
<contactref element="IN1" pad="G1"/>
<contactref element="RN40" pad="1"/>
<contactref element="RN42" pad="6"/>
<contactref element="FGPMMOPA6H" pad="03-GND"/>
<contactref element="FGPMMOPA6H" pad="08-GND"/>
<contactref element="FGPMMOPA6H" pad="12-GND"/>
<contactref element="FGPMMOPA6H" pad="19-GND"/>
<contactref element="R53" pad="1"/>
<contactref element="C58" pad="2"/>
<contactref element="C57" pad="2"/>
<contactref element="D54" pad="C"/>
<contactref element="C45" pad="-"/>
<contactref element="GPS-ANT" pad="GND@4"/>
<contactref element="GPS-ANT" pad="GND@2"/>
<contactref element="GPS-ANT" pad="GND@1"/>
<contactref element="GPS-ANT" pad="GND@3"/>
<contactref element="C61" pad="2"/>
<contactref element="1-9" pad="1"/>
<contactref element="+5VDC," pad="5"/>
<contactref element="+5VDC," pad="M1"/>
<contactref element="+5VDC," pad="M2"/>
<contactref element="P2" pad="31"/>
<contactref element="P2" pad="33"/>
<contactref element="P2" pad="27"/>
<contactref element="R55" pad="1"/>
<contactref element="SERIEL" pad="1"/>
<contactref element="R63" pad="2"/>
<contactref element="GROUND" pad="2"/>
<contactref element="GROUND" pad="1"/>
<contactref element="R64" pad="2"/>
<contactref element="EM-406A" pad="1"/>
<contactref element="GPS-FIX" pad="K"/>
<contactref element="C63" pad="2"/>
<contactref element="C64" pad="2"/>
<contactref element="MOD1016" pad="7"/>
</signal>
<signal name="+3V3">
<contactref element="ENC28J60" pad="15"/>
<contactref element="ENC28J60" pad="20"/>
<contactref element="ENC28J60" pad="19"/>
<contactref element="ENC28J60" pad="25"/>
<contactref element="ENC28J60" pad="28"/>
<contactref element="L40" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="LF33CV" pad="3"/>
<contactref element="C47" pad="1"/>
<contactref element="C48" pad="+"/>
<contactref element="L42" pad="2"/>
<contactref element="SERIEL" pad="4"/>
<contactref element="1-9" pad="2"/>
<contactref element="MOD1016" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="ENC28J60" pad="24"/>
<contactref element="C41" pad="1"/>
<contactref element="25MHZ" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="ENC28J60" pad="23"/>
<contactref element="C42" pad="1"/>
<contactref element="25MHZ" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R45" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="R44" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="ENC28J60" pad="12"/>
<contactref element="R45" pad="1"/>
<contactref element="HR911105A" pad="RD-"/>
</signal>
<signal name="N$5">
<contactref element="ENC28J60" pad="13"/>
<contactref element="R44" pad="1"/>
<contactref element="HR911105A" pad="RD+"/>
</signal>
<signal name="N$6">
<contactref element="R41" pad="2"/>
<contactref element="HR911105A" pad="G+"/>
</signal>
<signal name="N$7">
<contactref element="ENC28J60" pad="27"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="ENC28J60" pad="26"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R40" pad="2"/>
<contactref element="HR911105A" pad="Y+"/>
</signal>
<signal name="N$12">
<contactref element="ENC28J60" pad="17"/>
<contactref element="R43" pad="2"/>
<contactref element="HR911105A" pad="TD+"/>
</signal>
<signal name="N$13">
<contactref element="ENC28J60" pad="16"/>
<contactref element="R42" pad="1"/>
<contactref element="HR911105A" pad="TD-"/>
</signal>
<signal name="N$10">
<contactref element="R43" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="C40" pad="1"/>
<contactref element="L40" pad="1"/>
<contactref element="HR911105A" pad="P4"/>
</signal>
<signal name="N$11">
<contactref element="R46" pad="1"/>
<contactref element="ENC28J60" pad="14"/>
</signal>
<signal name="N$14">
<contactref element="ENC28J60" pad="1"/>
<contactref element="C44" pad="+"/>
</signal>
<signal name="+5V">
<contactref element="D47" pad="C"/>
<contactref element="D45" pad="C"/>
<contactref element="D41" pad="C"/>
<contactref element="D49" pad="C"/>
<contactref element="D43" pad="C"/>
<contactref element="D51" pad="C"/>
<contactref element="IN1" pad="3"/>
<contactref element="IN1" pad="6"/>
<contactref element="IN2" pad="6"/>
<contactref element="IN2" pad="3"/>
<contactref element="10-18" pad="8"/>
<contactref element="BUZZER" pad="+"/>
<contactref element="R54" pad="2"/>
<contactref element="R56" pad="2"/>
<contactref element="D53" pad="A"/>
<contactref element="LF33CV" pad="1"/>
<contactref element="C46" pad="1"/>
<contactref element="C45" pad="+"/>
<contactref element="L41" pad="1"/>
<contactref element="SERIEL" pad="5"/>
<contactref element="EM-406A" pad="2"/>
<contactref element="D52" pad="C"/>
<contactref element="P1" pad="43"/>
<contactref element="P1" pad="42"/>
</signal>
<signal name="N$15">
<contactref element="R47" pad="1"/>
<contactref element="ENC28J60" pad="10"/>
</signal>
<signal name="ENC28J60-SCK">
<contactref element="P1" pad="37"/>
<contactref element="ENC28J60" pad="8"/>
</signal>
<signal name="LCD-R/W">
<contactref element="P2" pad="36"/>
<contactref element="1-9" pad="5"/>
</signal>
<signal name="LCD-A0">
<contactref element="P2" pad="46"/>
<contactref element="1-9" pad="4"/>
</signal>
<signal name="LCD-D0">
<contactref element="P2" pad="16"/>
<contactref element="1-9" pad="7"/>
</signal>
<signal name="LCD-D1">
<contactref element="P2" pad="13"/>
<contactref element="1-9" pad="8"/>
</signal>
<signal name="LCD-D2">
<contactref element="P2" pad="14"/>
<contactref element="1-9" pad="9"/>
</signal>
<signal name="LCD-D4">
<contactref element="P1" pad="25"/>
<contactref element="10-18" pad="2"/>
</signal>
<signal name="LCD-D7">
<contactref element="P1" pad="28"/>
<contactref element="10-18" pad="5"/>
</signal>
<signal name="LCD-E1">
<contactref element="P2" pad="45"/>
<contactref element="1-9" pad="6"/>
</signal>
<signal name="LCD-D6">
<contactref element="P1" pad="27"/>
<contactref element="10-18" pad="4"/>
</signal>
<signal name="LCD-D3">
<contactref element="P2" pad="11"/>
<contactref element="10-18" pad="1"/>
</signal>
<signal name="IN2-A">
<contactref element="IN2" pad="7"/>
<contactref element="RN41" pad="11"/>
<contactref element="RN40" pad="2"/>
</signal>
<signal name="IN2-C">
<contactref element="IN2" pad="1"/>
<contactref element="RN41" pad="3"/>
<contactref element="RN40" pad="4"/>
</signal>
<signal name="IN2-B">
<contactref element="IN2" pad="4"/>
<contactref element="RN40" pad="3"/>
<contactref element="RN41" pad="9"/>
</signal>
<signal name="1.5V">
<contactref element="C56" pad="-"/>
<contactref element="C55" pad="+"/>
<contactref element="RN42" pad="1"/>
<contactref element="R62" pad="2"/>
<contactref element="R63" pad="1"/>
</signal>
<signal name="LCD-VEE">
<contactref element="1-9" pad="3"/>
<contactref element="D59" pad="A"/>
<contactref element="C63" pad="1"/>
</signal>
<signal name="+3V">
<contactref element="C56" pad="+"/>
<contactref element="P2" pad="5"/>
<contactref element="RN42" pad="5"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="GPS-1PPS">
<contactref element="EM-406A" pad="6"/>
<contactref element="P1" pad="11"/>
<contactref element="FGPMMOPA6H" pad="13-PPS"/>
<contactref element="P1" pad="35"/>
</signal>
<signal name="ENC28J60-CS">
<contactref element="P1" pad="36"/>
<contactref element="ENC28J60" pad="9"/>
</signal>
<signal name="LCD-LIGHT">
<contactref element="P2" pad="19"/>
<contactref element="R50" pad="2"/>
</signal>
<signal name="GPS-RX">
<contactref element="P1" pad="14"/>
<contactref element="R58" pad="1"/>
</signal>
<signal name="AMP1-RX">
<contactref element="IN1" pad="2"/>
<contactref element="P2" pad="47"/>
</signal>
<signal name="ENC28J60-SO">
<contactref element="ENC28J60" pad="6"/>
<contactref element="P1" pad="38"/>
</signal>
<signal name="N$34">
<contactref element="BUZZER" pad="-"/>
<contactref element="T41" pad="C"/>
<contactref element="R54" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="C50" pad="1"/>
<contactref element="RN41" pad="10"/>
</signal>
<signal name="AMP1-CH2">
<contactref element="P1" pad="20"/>
<contactref element="D47" pad="A"/>
<contactref element="D46" pad="C"/>
<contactref element="C53" pad="1"/>
<contactref element="RN42" pad="4"/>
</signal>
<signal name="AMP1-CH1">
<contactref element="P1" pad="19"/>
<contactref element="D45" pad="A"/>
<contactref element="D44" pad="C"/>
<contactref element="C54" pad="1"/>
<contactref element="RN42" pad="7"/>
</signal>
<signal name="AMP1-CH3">
<contactref element="P1" pad="7"/>
<contactref element="D41" pad="A"/>
<contactref element="D40" pad="C"/>
<contactref element="C52" pad="1"/>
<contactref element="RN42" pad="9"/>
</signal>
<signal name="AMP2-CH1">
<contactref element="P1" pad="22"/>
<contactref element="D50" pad="C"/>
<contactref element="D51" pad="A"/>
<contactref element="C51" pad="2"/>
<contactref element="RN42" pad="2"/>
</signal>
<signal name="AMP2-CH2">
<contactref element="P1" pad="21"/>
<contactref element="D49" pad="A"/>
<contactref element="D48" pad="C"/>
<contactref element="C50" pad="2"/>
<contactref element="RN42" pad="3"/>
</signal>
<signal name="AMP2-CH3">
<contactref element="P1" pad="10"/>
<contactref element="D43" pad="A"/>
<contactref element="D42" pad="C"/>
<contactref element="C49" pad="2"/>
<contactref element="RN42" pad="8"/>
</signal>
<signal name="IN1-B">
<contactref element="RN40" pad="7"/>
<contactref element="RN41" pad="6"/>
<contactref element="IN1" pad="4"/>
</signal>
<signal name="IN1-C">
<contactref element="IN1" pad="1"/>
<contactref element="RN40" pad="9"/>
<contactref element="RN41" pad="2"/>
</signal>
<signal name="N$46">
<contactref element="RN41" pad="12"/>
<contactref element="C51" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="RN41" pad="5"/>
<contactref element="C53" pad="2"/>
</signal>
<signal name="N$67">
<contactref element="C52" pad="2"/>
<contactref element="RN41" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="C54" pad="2"/>
<contactref element="RN41" pad="7"/>
</signal>
<signal name="N$64">
<contactref element="C49" pad="1"/>
<contactref element="RN41" pad="4"/>
</signal>
<signal name="IN1-A">
<contactref element="RN40" pad="6"/>
<contactref element="RN41" pad="8"/>
<contactref element="IN1" pad="7"/>
</signal>
<signal name="LCD-D5">
<contactref element="P1" pad="26"/>
<contactref element="10-18" pad="3"/>
</signal>
<signal name="N$52">
<contactref element="GPS-ANT" pad="SIG"/>
<contactref element="FGPMMOPA6H" pad="11-EXA"/>
</signal>
<signal name="GPS-TX">
<contactref element="P2" pad="30"/>
<contactref element="R59" pad="1"/>
</signal>
<signal name="BUZZER">
<contactref element="P1" pad="15"/>
<contactref element="R52" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="R53" pad="2"/>
<contactref element="T41" pad="B"/>
<contactref element="R52" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="C60" pad="2"/>
<contactref element="D54" pad="A"/>
<contactref element="D55" pad="C"/>
</signal>
<signal name="N$44">
<contactref element="C58" pad="1"/>
<contactref element="D55" pad="A"/>
<contactref element="D56" pad="C"/>
</signal>
<signal name="N$50">
<contactref element="D56" pad="A"/>
<contactref element="D57" pad="C"/>
<contactref element="C59" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="FGPMMOPA6H" pad="05-3DF"/>
<contactref element="R57" pad="1"/>
</signal>
<signal name="ENC28J60-INT">
<contactref element="ENC28J60" pad="4"/>
<contactref element="P2" pad="9"/>
</signal>
<signal name="N$20">
<contactref element="C60" pad="1"/>
<contactref element="R51" pad="2"/>
<contactref element="C59" pad="1"/>
<contactref element="C62" pad="1"/>
</signal>
<signal name="LCD-CONTRAST">
<contactref element="P2" pad="25"/>
<contactref element="R51" pad="1"/>
<contactref element="P2" pad="26"/>
</signal>
<signal name="N$30">
<contactref element="R50" pad="1"/>
<contactref element="T40" pad="B"/>
</signal>
<signal name="LCD-E2">
<contactref element="P2" pad="43"/>
<contactref element="10-18" pad="6"/>
</signal>
<signal name="LCD-RES">
<contactref element="10-18" pad="7"/>
<contactref element="P2" pad="24"/>
</signal>
<signal name="LCD-C">
<contactref element="10-18" pad="9"/>
<contactref element="R48" pad="2"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="ENC28J60-SI">
<contactref element="ENC28J60" pad="7"/>
<contactref element="P1" pad="39"/>
</signal>
<signal name="AMP1-TX">
<contactref element="IN1" pad="8"/>
<contactref element="P2" pad="34"/>
</signal>
<signal name="POWER-CRTL">
<contactref element="R55" pad="2"/>
<contactref element="R56" pad="1"/>
<contactref element="P1" pad="13"/>
</signal>
<signal name="N$16,">
<contactref element="EM-406A" pad="3"/>
<contactref element="FGPMMOPA6H" pad="10-RX"/>
<contactref element="R58" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="EM-406A" pad="4"/>
<contactref element="FGPMMOPA6H" pad="09-TX"/>
<contactref element="R59" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R60" pad="1"/>
<contactref element="SERIEL" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="R61" pad="1"/>
<contactref element="SERIEL" pad="2"/>
</signal>
<signal name="N$25,">
<contactref element="FGPMMOPA6H" pad="01-VCC"/>
<contactref element="C61" pad="1"/>
<contactref element="L42" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="T40" pad="C"/>
<contactref element="JP1" pad="2"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="JP1" pad="1"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="+5VDC," pad="1"/>
<contactref element="L41" pad="2"/>
<contactref element="C64" pad="1"/>
</signal>
<signal name="SERIAL-TX">
<contactref element="P2" pad="38"/>
<contactref element="R60" pad="2"/>
</signal>
<signal name="AMP2-TX">
<contactref element="P1" pad="41"/>
<contactref element="IN2" pad="8"/>
</signal>
<signal name="SERIAL-RX">
<contactref element="P2" pad="37"/>
<contactref element="R61" pad="2"/>
</signal>
<signal name="AMP2-RX">
<contactref element="P1" pad="40"/>
<contactref element="IN2" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="HR911105A" pad="NC"/>
<contactref element="D52" pad="A"/>
</signal>
<signal name="PC0">
<contactref element="P1" pad="8"/>
<contactref element="R65" pad="2"/>
<contactref element="R64" pad="1"/>
</signal>
<signal name="MP">
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="P2" pad="3"/>
<contactref element="P2" pad="4"/>
<contactref element="D53" pad="C"/>
</signal>
<signal name="N$16">
<contactref element="R57" pad="2"/>
<contactref element="GPS-FIX" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="D58" pad="A"/>
<contactref element="D59" pad="C"/>
<contactref element="C62" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="D57" pad="A"/>
<contactref element="C57" pad="1"/>
<contactref element="D58" pad="C"/>
</signal>
<signal name="PB9-SDA">
<contactref element="P2" pad="20"/>
<contactref element="MOD1016" pad="6"/>
</signal>
<signal name="PB6-SCL">
<contactref element="MOD1016" pad="4"/>
<contactref element="P2" pad="23"/>
</signal>
<signal name="PC15-IRQ">
<contactref element="MOD1016" pad="3"/>
<contactref element="P2" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
